|  |  |  |
| --- | --- | --- |
| **cemark**  **RI.SE 0402** |  | *CE marking, consisting of the “CE”-symbol*  *Identification number of the notified test laboratory* |
| **AnyCo Ltd, PO Box 21, B-1050, Brussels, Belgium**  **18**  00001-CPR-2013/05/12 |  | *name and the registered address of the manufacturer, or identifying mark*  *Last two digits of the year in which the marking was first affixed*  *Reference number of the DoP* |
| **EN 13241-1:2003+A2:2016**  Product A  intended to be used in (e.g. curtain walling, fire compartmentation, etc.)  **water thightness:** Class:  **resistance to wind load:** Class:  **thermal resistance:** W/m2K  **air permeability:** Class:  **Dangerous substances:** Pass  **Safe opening:** Pass  **Definition of geometry of glass components:** Pass  **Mechanical resistance & stability:** Pass **Operating forces (power operated doors)** < 400N  **Durability of water tightness, thermal resistance & air permeability:** 100.000 cycles |  | *No. of European standard applied, as referenced in OJEU (see note 14)*  *Unique identification code of the product-type*  *Intended use of the product as laid down in the European standard applied*  *Level or class of the performance declared* |

|  |
| --- |
| **Power operated doors also compliance:** |
| 2006/42/EC (MD) |
| 2014/30/EU (EMCD) |